Wiring Diagrams
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Conventional Heating and Cooling (Up to 2 Stages each)



[image: ][image: ]Heat Pump (air or geothermal) With Auxiliary Heat 

Heat Pump with Auxiliary Heat and no C wire (Using PEK) 
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Accessory Devices
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Boiler or radiant system with air handler
and conventional cooling or heat pump
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Note: Do not jumper Re or Rh,
ecobee3 does this automatically.
R can go into either Rc or Rh
terminals on your ecobee3.
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Accessory devices

The ecobee3 can control an accessory HVAC device like a
humidifier, dehumidifier, or ventilation device from its ACC
terminals.

If you have 2 wires at the thermostat from the accessory,
then your accessory is externally powered. If you have only 1
wire then it is internally powered.
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Note: You will need to configure the accessory device when you
first power on your ecobee3.
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Conventional heating and cooling
(up to 2 stages each)
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Air conditioner Furnace
Stage 2 heat and coo Note: Do not jumper Re or Rh,
if applicable ecobee3 does this automatically.

R can go into either Rc or Rh
terminals on your ecobees.
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Heat pump (air or geothermal)

with auxiliary heat
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Heat pump Air handler

Stage 2 compressor and
auxiliary heat if applicable

Note: Do not jumper Re or Rh,
ecobee3 does this automatically.
R can go into either Rc or Rh
terminals on your ecobee3.
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